Firmware Update – ASM2464PD

The firmware update is only suitable for the following model: 40Gbps Enclosure

Step as follows.

1. Connect the enclosure with the SSD built-in to the PC.
2. Open file\Mptols For ASM246PD for std\20250801\_ASM246xMPTool\_v1.0.3.2\ ASM246xMPTool.exe
3. Check if the update tool has detected the enclosure and displays it on scree.



Password : asmedia



Click “FW Browser” to loading fw file(AS\_USB4\_250528\_85\_00\_00) and click  to start.

The update tool is already set correctly, do not change the settings.

4. Click Update Device button.

5. After the update tool displays “Pass” message, safely remove the enclosure via “Safely Remove hardware and Eject Media” menu.

6. Disconnect the USB cable from the PC.

7. Connect the enclosure to the PC again