April 2022 Update

Note: The update resolves intermittent mounting issues in Windows.

1. Unzip the contents of the zip file. 
2. Right-click ASM105xMPTool.exe and select Run As Administrator. (If it does not open, right click the file, select Properties, then Unblock).
3. Connect the Novus to your computer. The drive should appear in the Port 0 row within the application. 
4. Click the Play button in the lower left corner. The update will process. It will display PASS if the update completes successfully. 
5. Eject the Novus and then turn the power off and back on. The process is now complete.

