**Update Procedure：**  
1. Ready a laptop with Type-C port, run “ASM246xMPTool.exe”;

1. Click this icon to unlock ，and input password: “asmedia”;
2. Under the section “Device Functions”(located on right), select the option of “Update FW” 
3. Select where the firmware is located 
4. Click  button (located at bottom left corner), the update shall start.
5. Update is successful is there is notification message showing “PASS”.

